
             ----------------------------------------------------
                         Precision MicroControl Corp.
                      MFX-PCI Firmware Revision History
               Copyright 2002-2014 Precision MicroControl Corp.
               $Id: revision.txt 36 2014-09-12 22:30:32Z brian $
             ----------------------------------------------------


                        CONFIDENTIAL AND PROPRIETARY:
This file contains confidential and proprietary information that is the sole
property of Precision MicroControl Corp. This confidential information is
not to be copied, disclosed or reproduced in whole or in part by any means
(including photocopying or storage in an information storage/retrieval
system) or transmitted in any form or by any means except as authorized by
written contract with Precision MicroControl Corp. 


Changes for Rev. 0.3a
===============================================================================
 10/18/02  Implemented Output Mode command for steppers and servos.
 10/21/02  Re-organized status words to accomodate host interrupts.

Changes for Rev. 0.4a
===============================================================================
 10/22/02  Implemented host communication interrupts.

Changes for Rev. 0.5a
===============================================================================
 10/22/02  Implemented host motor status interrupts.

Changes for Rev. 0.6a
===============================================================================
 10/24/02  Implemented closed loop stepper mode.
 10/24/02  Connected encoder error inputs to motor status.
 10/24/02  Readjusted stepper internal feedback loop gain to 0.0005. This
            matches FPGA 40 MHz clock rate.
 10/25/02  Fixed stepper beakpoint. Previous code was setting breakpoint enable
            bit in the FPGA mode register instead of the control register.

Changes for Rev. 0.7a
===============================================================================
 10/28/02  Added code to enable watchdog circuit. Use DW command to disable.

Changes for Rev. 0.8a
===============================================================================
 10/29/02  Modified code to support 8 axes.
 11/1/02   Modified code that updates target position after an axis is
           commanded to stop. New code updates target position and target
           count after profiler signals trajectory complete. For stepper
           motors, the target update occurs after pulses are actually turned
           off. See code in LINPATH.C and MODECMD.C - pm().
 11/1/02   Added code to RT command to reset DAC's and FPGA.

Changes for Rev. 0.9a
===============================================================================
 11/15/02  Modified DAC interface circuit in FPGA to generate a DAC clock
           signal of 10MHz. Running the DAC at 20 MHz resulted in unreliable
           writes to channel 2.
 11/18/02  Fixed define for auxiliary encoder index enable in MOTIFC.H
           Correct value for AUXIDXENA is 0x1000
 11/18/02  Corrected code for Abort (AB) command.
 11/18/02  Corrected code for Output mode for Compare (OC) command
 11/18/02  Changed stepper pulse generator circuit in FPGA to provide
           increased resolution. Maximum step rate from FPGA is now 10MHz.
           The range of the parameter to the Set Torque command for a
           stepper is 0 to 10. This produces a step frequency of 0 to 10 MHz.
           To match this, the stepper calibration value in MOTSVC.C is 50000,
           and the proportional gain setting is 0.001.

Changes for Rev. 0.9b
===============================================================================
 11/19/02  Implemented RT command to restart software on board. Added support
           for 3 different parameters. A parameter of 0 with the RT command will
           result in the kernel and motion control software being restarted.
           A parameter of -1 will restart the boot loader firmware. A parameter
           of -2 will generate a memory exception which will pass control to the
           debug monitor.
 11/19/02  Added code to release I/O reset signal after initializing FPGA. This
           is required for DAC's to operate.

Changes for Rev. 0.9c
===============================================================================
 11/19/02  Modified code for Position Record command in tellcmd.c so that
           interrupts are disabled while recording is initiated on all selected
           axes. This insures recorded data is synchronized for all axes.
 11/19/02  Implemented Display recorded motor status command (DD, code=256).
 11/19/02  Implemented digital I/O channel commands.

Changes for Rev. 0.9d
===============================================================================
 11/20/02  Fixed Wait for Position commands. Macro load_primary_compare_register()
           in motifc.h was not defined. Cleaned up code in ccbcmd.c.

Changes for Rev. 0.9e
===============================================================================
 11/25/02  Implemented analog input commands.
 
Changes for Rev. 0.9f
===============================================================================
 11/25/02  Enabled synchronized reading of encoders in FPGA. Encoder and stepper
           counters latch position on rising edge of timer interrupt signal.
           Timer0 uses Pulse Generator mode as setup in CPU_ASM.S.
 11/25/02  Corrected addresses of beginning and end of firmware in START.S.
 12/3/02   Cleaned up initialization of stepper motor parameters. Set gain of
           pulse generator for stepper in open loop mode to 0.0001.

Changes for Rev. 0.9g
===============================================================================
 12/6/02   Optimized position counters in FPGA to allow for capture and compare
           feature on all servo and stepper axes. Capture function now uses
           index registers, so capture can't be performed while indexing
           a motor.
 12/6/02   Modified pulse generator in FPGA to allow full 0 to 65535 input
           value. Changed value of STEPPER_MAX_OUTPUT_UNITS constant to 65535.

Changes for Rev. 0.9h
===============================================================================
 12/9/02   Enabled processing of Contour Path commands. Previous code had
           CP commands disabled in CMDEXE.C.
 12/9/02   Modified contouring code so that motion table is the same size for
           all axes. In other PMC products, motion table has 256 blocks for
           axis 1, but only 16 blocks for all other axes. In order to simplify
           and enhance contouring mode, all axes now have 256 blocks in the
           motion table.
 12/9/02   Increase number of supported RAM macros to 1000. Previous code only
           allowed macros 10 through 255 to be defined. New code allows macros
           0 through 999 to be defined. These macros are placed in RAM and will
           be lost when the motion controller is reset.
 12/10/02  Fixed Wait for Index command for open loop steppers. Previous code
           was incorrectly monitoring MTRAEI flag. When closed loop stepper
           mode is selected, encoder input is fed to primary counter in FPGA
           and MTRIDX flag indicates when index has occured. Also fixed
           setting of MTRAXF flag in MOTUPD.C. Previous code set flag in motor
           table status instead of local status variable that is written over
           motor table variable.
 12/11/02  Modified code to clear Encoder Fault flags in status when motor on
           command is issued.
 12/11/02  Modified axis I/O code so that outputs are numbered 33 through 64.
           This matches channel numbers used in digital I/O commands.
 12/12/02  Added Model Number to board configuration data structure. Changed
           VE command code to include model number in dispaly. Changed
           product name to DC44-PCIXXXX-O where XXXX is model number, O is
           option designator.
           
Changes for Rev. 1.0a
===============================================================================
 12/13/02  Changed product name to MFX-PCI. Version command now displays
           name MFX-PCIXXXX-O where XXXX is model number, O is hardware option
           designator.
 12/26/02  Included 2 different FPGA configuration data sets. The model
           number that is stored in the Firmware configuration data in the
           Flash memory determines which FPGA data is loaded. See
           init_registers() in INIT.C.
 12/26/02  Increased value of constant that specifies the amount of memory
           available on the board. This value is used to locate the initial
           processor stack. In previous code HARD_CODED_MEM_SIZE was set to
           0x100000 in START.S. New code has it set to 0x400000 which is
           safe for both MFX-PCI and DCX-PCI boards.
           
           
Changes for Rev. 1.0b
===============================================================================
 1/13/03   Inverted optically isolated inputs in FPGA circuits. Channel
           commands will report state of these inputs as 0 when configured
           as default active high and have no input current.

 1/13/03   Corrected command table so Velocity Override command can accept
           real parameters.

 1/13/03   Corrected code for Delay at Target command. Previous code multiplied
           command parameter by MOTOR_UPDATES_PER_SEC which is 4 times greater
           than delay timer is actually updated.

 1/14/03   Added ability to read encoder fault word to Tell Status command.
           TS with a parameter value of 160 will display the encoder fault
           word as a 32 bit unsigned integer. Parameter values 161 to 191
           will display the state of encoder fault bits 1 to 31 respectively.

 1/14/03   Added code to record auxiliary encoder position for stepper axes.
           Implemented Display recorded Auxiliary position command (DA, code=219).

 1/14/03   Implemented Reset of a specific axis with the RT command. If an axis
           is specified when the RT command is issued, only that axis will be
           reset.

 1/15/03   Added Memory Allocate (ME), Free Memory (FM), and Memory Display (DE)
           commands. The ME command allocates the amount memory specified by
           the command parameter and places the address of the memory in user
           register 0. If the specified amount of memory can't be allocated,
           a value of 0 is placed in user register 0. The parameter to the FM
           command should be the address of the memory to be freed. This must
           be the address of memory that was allocated with the ME command.
           The parameter to the DE command is any valid physical address.
           If an axis is specified with the DE command, the entire motor table
           for that axis will be displayed. The DE command can only be issued
           to an ASCII interface.

 1/15/03   Made Help command display consistent with MCCL reference manual list
           of commands.

 1/15/03   Implemented command help. Typing HE"mm" where mm is a valid command
           mnemonic will display addition help information for that command.

 1/15/03   Modified Set Velocity command code so that the minimum velocity for
           a stepper axis will always be equal to or less than the maximum velocity.

 1/16/03   Implemented Information Display command (ID, code = 218). This command
           is only valid for the ASCII interface and generates formatted
           displays. The ID command must be issued to a specific axis and takes
           the following parameters:
              Parameter      Return Value
           ===========================================
                 0       show status information
                 1       show auxiliary status information
                 2       show motor table information
                 3       show internal motor table information
                 4       show filter gains, command output
                 5       show encoder fault inputs and enable bits
                 6       show axis I/O assignments

 1/16/03   Removed formatted displays form the Tell Status command.


Changes for Rev. 1.0c
===============================================================================
 1/17/03   Corrected which status bit is used to indicated when an open loop
           stepper axis is looking for edge (home). Previous code used bit 23
           to indicated Looking for Edge. New code uses bit 17.

 1/17/03   Modified operation of status bits related to indexing or homing
           a servo or stepper axis.

           For a servo axis (or stepper in closed loop mode), the following table
           shows the state of the motor status bits after each of the commands
           in an indexing operation:

                      Index Arm   (index occurs)   Wait for Index   Motor On
  =============================================================================
     Encoder Index        0              1               1             ?
   Looking for Index      1              1               0             0
      Index Found         0              1               1             0
        Homed             0              0               0             1

           Note that a homing sequence should test for the Index Found status
           bit to be set before issuing the Wait for Index command.

           For a stepper axis in open loop mode, the following table shows the
           state of the motor status bits after each of the commands in a
           homing operation:

                      Edge Latch  (home occurs)   Wait for Edge   Motor On
  =============================================================================
     Stepper Home         0              1               1             ?
   Looking for Edge       1              1               0             0
      Edge Found          0              1               1             0
        Homed             0              0               0             1

 1/17/03   Added code to Input Mode command to clear homing and indexing status
           bits when switching a stepper between open and closed loop modes.

 1/20/03   Added inverter to CLR input of JK flip-flop in FPGA encoder capture
           circuits. In previous code, FPGA encoder capture circuits were
           permanently disabled.

 1/20/03   Fixed capture and compare commands so they can be used for both
           open and closed loop steppers. In previous code they were disabled
           for closed loop steppers.

 1/20/03   Modified code so that value returned by Auxiliary Tell and Display
           recorded Auxiliary commands takes into account current Auxiliary
           Index and Auxiliary Offset values.

 1/20/03   Cleaned up operation of status bits for auxiliary encoder indexing.
           Corrected code so that Auxiliary Home and Auxiliary Find index
           commands can be issued without specifying an axis.


Changes for Rev. 1.0d
===============================================================================
 1/23/03   Moved Motor table and Point data to cached memory for faster motor
           update processing.

 1/23/03   Modified hostint() function so that processor interrupts are only
           disabled if host interrupt needs to be generated. This will
           reduce the amount of time that interrupts are disabled.


Changes for Rev. 1.0e
===============================================================================
 1/29/03   Modified code for Tell Analog and Get Analog commands so that analog
           reading is correct. In previous code, command had to be issued 3
           times to the same channel to get the current analog reading. Also
           changed "value" variable from short to integer so that replies
           over the binary interface are correct.


Changes for Rev. 1.0f
===============================================================================
 2/12/03   Changed Timer 0 output high duration to 50 microseconds. This
           makes the interrupt service time easier to measure with an
           oscilloscope. See init_timer0() in cpu_asm.S.

 2/12/03   Added code to set initial floating point context for new tasks
           under RTEMS. New code sets FS bit in coprocessor control and status
           register. This prevents unwanted exceptions on underflow and
           inexact results. See _CPU_Initialize() in cpu.c.

 2/12/03   Added code to lock first 4 kilobytes of PMON code into processor
           instruction cache. This includes interrupt service code that is
           running out of FLASH memory. In previous code, when a background
           task forced the interrupt service code out of cache, the interrupt
           service would execute out of slow flash memory and add an extra 60
           microseconds to the interrupt service time. See start.S.


Changes for Rev. 1.1a
===============================================================================
 2/20/03   Implemented Position Compare feature in firmware. This feature
           provides the same funtionality as the implemention on the DCX-PCI300
           product except that all axis compare outputs are or'd together and
           are connected to output channel 33. Also the Oneshot period accuracy
           is limited to +/-1 millisecond.

 2/24/03   Fixed miss spelling of "variable" in Help command display. Added
           "ID" mnemonic to Help command display under reporting commands.
 
 2/25/03   Increased maximum number of tasks in SYSTEM.H file to 13. This allows
           up to 10 background tasks to be created with the Generate Task
           command.

 4/1/03    Modified code for point to point moves in trapezoidal mode. New code
           holds speed of stepper axis at minimum velocity until motor reaches
           target. In previous code, trajectory generator was disabled and
           velocity set to zero when optimal position was within one update of
           reaching target. This criteria for stopping should only be applied
           to servo axes.

 4/2/03    Modifed stepper pulse generator circuit in FPGA. In new design,
           internal registers are cleared when pulses are first enabled. This
           results in immediate output of pulses. Also modified circuit to
           invert output of pulse divider so that output pulse is immediate.
           In previous design, pulse output could be delayed for up to one
           pulse period after they were enabled.

 4/3/03    Modified code for Set Velocity and Minimum Velocity commands so
           that profile generator minveloc variable is set to the minimum
           of the max and min programmed velocities. This only applies
           to stepper axes and insures that the minimum velocity is a
           acceptable value (ie. less than maximum).


Changes for Rev. 1.2a
===============================================================================
 5/2/03    Set hard coded memory size to 16 megabytes. This is the available
           RAM on the MFX-PCI. See HARD_CODED_MEM_SIZE constant in START.S. 
           
 5/2/03    Increased heap size to 8 megabytes (see LIBC_HEAP_SIZE in BSPSTART.C).
           The code in bsp_start() sets the RTEMS Workspace memory to
           follow the heap. Enabled memory allocation statistics in MALLOC.C.
           The available heap memory will be displayed after the macros when
           the Tell Macro command is issued.
 
 5/2/03    Switch on-board file system from MINI IMFS to IMFS to support
           network interface. See CONFIGURE_USE_IMFS_AS_BASE_FILESYSTEM in
           SYSTEM.H file.
           
 5/2/03    Built in network interface support: TCP/IP through ethernet LAN.
           BSD network task priority is set to 50.
           This is only used when the MFX board is run standalone.

 5/14/03   Created version of CONSOLE.C that perform serial I/O via direct
           access to TX49 serial port registers. This is only used when
           the MFX board is run standalone.

 5/14/03   Built in RTEMS monitor. Initiated by issuing "RT-3" MCCL command.
           At "RTEMS>" prompt, type help for further instructions. Added
           stack address, stack size and register storage address to "TASK"
           command dump.

 5/16/03   Cleaned up CPU_ASM.S. Added ".set noreorder/reorder" directives around
           all critical code in this module. Removed jump to _ISR_Handler_prom_exit
           when interrupt source can't be determined (this was incorrect code).

 5/19/03   Added extra input buffering to telnet ASCII interface server. This
           allows telnet clients that send one character at a time to work
           correctly.

 5/21/03   Changed MFXPCI application source code files from Windows style CR-LF
           termination to Unix style LF termination. Also did the same for
           compiler "specs" file (/usr/local/lib/mips-ecoff/2.95.2/specs).
           This was required to get RTEMS to build under CYGWIN on Windows XP.

 5/21/03   Modified PATH statement in Build script to:
               PATH=/usr/local/bin/mips-ecoff:/usr/local/bin:/usr/bin:/bin
           This insures cross-development tools are used before native tools.

 5/22/03   Added call to Untar_FromMemory() in init.c to create root filesystem.
	   
 5/22/03   Built in Web server. Modified distibution code to use RTEMS timer
           routines instead of POSIX. Declared "tp" variable in webmain.c to
           be "static" to prevent conflict with tp() function.
	   
 5/27/03   Copied newer Web server code from RTEMS 4.6.0. Note that new *.h
           files are copied into build directory. The makefiles in the build
           directory are modified to build the new modules. 

 5/28/03   Copied newer FTP server code from RTEMS 4.6.0. Note that new *.h
           files are copied into build directory. Defeated code that
           maintains a separate environment for each FTP login. This feature
           isn't supported by current libc code. Changed snprintf() calls
           in webmain.c to sprintf(). The safer snprintf() function isn't
           implemented in the newlib that is currently being used.

 5/29/03   Added code to calculate the size of root file system image in call
           to Untar_FromMemory() in init.c.

 5/30/03   Implemented Network Binary Command Interface Server. This server
           waits on port 9100 of the TCP/IP stack and processes packets
           containing binary formated MCCL commands.

 6/3/03    Corrected code in start.S that flushes data and code caches after
           moving firmware from extra flash device (U38) into RAM. This is
           only used for stanalone operation.


Changes for Rev. 2.0a
===============================================================================
 6/5/03    Added use_PCI_interface, use_serial_interface and use_network_interface
           constants to board.h to allow selecting which interfaces are built
           into code.

 6/5/03    Moved Interrupt_7_isr() function into init.c to prevent NE2000 driver
           code (and thus networking code) from being included in build if
           use_network_interface is undefined.

 6/11/03   Added support for 1040 version of MFX-PCI product. This version has
           only stepper axes numbered 1 through 4. Changed motor update code
           to properly service stepper modules regardless of whether they are
           numbered 5 through 8, or 1 through 4. Added code to set num_of_motors
           variable from Flash configuration data.

 6/12/03   Added code to determine "option" value for product number displayed
           by Version command. The option value is based on hardware present
           on the board and features supported in firmware.

 6/16/03   Changed firmware link commands in LINKCMDS file to cause a copy
           of initialized data sections to be placed after text sections. Added
           code to initialize data sections from this copy in the startup
           code. 
	   
 6/16/03   Corrected encoder error input masks for new MFX-PCI connector
           scheme. Odd numbered axes have encoder error detection on A, B and
           Z inputs individually, plus global detection for any of the inputs.
           Even numbered axes have only have global detection.
	   
 6/16/03   Corrected code in motor update that called set_cmd_out() instead of
           set_cmd_output() to set command output to 0 if maximum following
           error exceeded. The macro set_cmd_out() is only used for servos.
           The function set_cmd_output() determines which macro to call
           based on axis type (servo or stepper).


Changes for Rev. 2.0b
===============================================================================
 9/26/03   Corrected Wait command time period when executed in a background task.
           In previous code Wait command completed in one forth the specified
           period. New code defines CLOCK_UPDATES_PER_SEC as 4000 and
           MOTOR_UPDATES_PER_SEC as 1000. The latter being how often each
           motor is serviced (ie. checked for errors).


Changes for Rev. 2.0c
===============================================================================
 10/1/03   Changed FPGA configurations so that Capture Inputs and Compare
           Outputs of DCX-PCI1440 and DCX-PCI1040 match the connector pin
           assignments given in the User's Manual.


Changes for Rev. 2.0d
===============================================================================
 10/4/03   Changed profile generator code so that stepper motors in contour
           mode have their trajectory complete bit set when move is completed.

 10/6/03   Added code to clear motor At Target bit for servos in contour mode
           moving with trapezoidal velocity profile. Removed code that caused
           steppers in contour mode to have their Motor At Target bit to be
           set during motor update.

 10/7/03   Added code to disable following error 1 count deadband for stepper
           motors if motor is not moving. This deadband reduces frequency gitter
           of stepper motors, but caused motor to stall short of target in
           previous code.

 10/8/03   Added code to linear path generator to zero feed-forward variable
           when a stepper motor completes a move. This corrects a problem with
           stepper motors when they are switched to contour mode. In previous
           code, residual feed-forward value would cause a stepper motor to
           move slightly when it was placed in contour mode.

	   
Changes for Rev. 2.1a
===============================================================================
 1/20/04   Replaced FPGA configuration files for MFX-PCI1440 and MFX-PCI1040
           products. New versions are implemented in Verilog hardware
           definition language (HDL). Previous FPGA designs were schematic
           based. The FPGA design in MFX-PCI1441 is still schematic based.

	   
Changes for Rev. 2.1b
===============================================================================
  2/6/04   Modified the way profile 'stop' flag functions. In new code, if an
           axis is commanded to stop, the flag will be set and remain set
           until the start of the next motion. This was done to allow all
           contouring axes to recognize when they were commanded to stop
           (requiring them to update their target positions). In order to
           implement this, stop flag is cleared before starting motion in
	   position, velocity and contouring modes. This fixes a problem in
	   previous code where contouring axes could not be moved after being
	   commanded to stop. Also removed code that cleared stop flag at the
           end of position mode moves. As a backup, added code to clear the
           stop flag when motor off command is executed. Added code to
	   update the target position of motors in contour mode that are
	   commanded to stop. Also changed motor on command so that it does not
	   disable pulses for stepper axes that are in contouring mode (these
	   axes need pulses enabled).


Changes for Rev. 2.1c
===============================================================================
 2/24/04   Added error checking in get_task_data() function to check for
           valid task data. Function will return 0 if task or dats is invalid.
	   This will cause the Escape Task command to return and error code
	   of -20 if task doesn't exist.
	   
 2/24/04   Added code to clear index and auxiliary index status flags in Index
           Arm (IA) and Auxiliary Find index (AF) commands. This enables status
           change detection in motor update service. In previous code, index
           found status would not be set if Index Arm command was issued and
           index input was already active. Similarly, for Auxiliary encoder
           index found status and Auxiliary Find index command. Code was
           correct for Find Index, Find Edge and Edge Latch commands.


Changes for Rev. 2.2a
===============================================================================
 4/14/04   Modified code so that the active level of amplifier enable outputs
           can be inverted with the Channel High and Channel Low commands.
           The Reset command for an axis will set the amplifier enable output
           to its' default inactive level and reset the digital output invert
           flag.


Changes for Rev. 2.3a
===============================================================================
 5/19/04   Increased the number of Global User Registers by 744.
           In the new firmware there are 990 global registers, numbered
           10 - 999. There are still 10 Local User Registers, numbered 0 - 9,
           available for each foreground and background task.

 5/19/04   Increased the number of macros that can be created by 976. In the
           new firmware 2000 macros numbered 0 to 1999 can be created.

 5/19/04   Added a new option to the Information Display (ID) command to show
           the active background tasks. With a parameter of 7, the ID command
           will show a list of ID's for the currently running background tasks.
           The ID's will be in decimal or hexidecimal format based on the
           current mode.


Changes for Rev. 2.3b
===============================================================================
 8/13/04   Added code to disable breakpoint latch when stepper axes are placed
           in slave mode. Also added code in motor_update_service function to
           enable and disable pulses for steppers in slave mode. Added code
           in set_cmd_output function to set direction output for steppers in
           slave mode. In previous code, stepper motors had to be in contour
           mode prior to being placed in slave mode to work correctly. 


Changes for Rev. 2.4a
===============================================================================
 8/17/04   Implemented crossover of position error and feed-forward terms
           between 2 axes. When the position error crossover is enabled for
           an axis, the position error of another axis will be subtracted
           or added from the axes' position error. The modified position error
           is then used as the input to the PID calculations. When the feed-
           forward crossover is enabled for an axis, the feed-forward terms
           of another axis will be added or subtracted from the axes' output
           command. This feature is only available for servo axes. For optimal
           operation, the axis for which crossovers are enabled should be the
           higher numbered axis.
           
           To enable position error crossover, use the Look Up (LU) command 
           to determine the offset of the "crosserraxis" variable. Use the
           Write Word (WW) command to set this word variable (16 bit) for the
           target axis to the axis number of the crossover axis. To invert
           the sign of the crossover position error, set the variable to the
           negative axis number.
           
           To enable feed-forward crossover, use the Look Up (LU) command
           to determine the offset of the "crossffaxis" variable. Use the
           Write Word (WW) command to set this word variable (16 bit) for the
           target axis to the axis number of the crossover axis. To invert
           the sign of the crossover feed-forward terms, set the variable to
           the negative axis number.
           
           Example MCCL commands:
               Assume Y is axis 1, X is axis 2, X is mechanically linked so it moves when Y moves

               LU"crosserraxis",AR5     ; Lookup "crosserraxis" variable offset, move to user register 5
               AL1,2WW@5                ; Write axis 1 specifier to axis 2 variable (variable offset in register 5)
                                        ;   X axis error = X axis error - Y axis error
                or 
               AL-1,2WW@5               ; Write negative axis 1 specifier to axis 2 variable (position error will be added)
                                        ;   X axis error = X axis error + Y axis error


               LU"crossffaxis",AR5     ; Lookup "crossffaxis" variable offset, move to user register 5
               AL1,2WW@5                ; Write axis 1 specifier to axis 2 variable (variable offset in register 5)
                                        ;   X command output = X feed-forward terms + Y feed-forward terms
                or 
               AL-1,2WW@5               ; Write negative axis 1 specifier to axis 2 variable (feed-forward will be subtracted)
                                        ;   X command output = X feed-forward terms - Y feed-forward terms
                                        
           Note that if the axis for which crossovers are enable has the
           lower axis number, the position error and the feed-forward terms
           that is taken from the other axis will be from the previous
           motor update period. In this case, the position error readings
           and the feed-forward terms of the 2 axes will not be synchronized.
           This will result in less than optimal operation of the axis on
           which crossovers are enabled.


Changes for Rev. 2.5a
===============================================================================
 8/24/04   Removed implementation of feed-forward crossover feature and
           replaced it with command signal crossover feature.
           
           When the command signal crossover is enabled for an axis, the
           command signal (which incluides the PID and feed-forward terms)
           of another axis will be added or subtracted from the axes' output
           command. This feature is only available for servo axes. For optimal
           operation, the axis for which crossovers are enabled should be the
           higher numbered axis.
           
           To enable command signal crossover, use the Look Up (LU) command
           to determine the offset of the "crosscmdaxis" variable. Use the
           Write Word (WW) command to set this word variable (16 bit) for the
           target axis to the axis number of the crossover axis. To invert
           the sign of the crossover command signal, set the variable to
           the negative axis number.
           
           Example MCCL commands:
               Assume Y is axis 1, X is axis 2, X is mechanically linked so it moves when Y moves

               LU"crosscmdaxis",AR5     ; Lookup "crosscmdaxis" variable offset, move to user register 5
               AL1,2WW@5                ; Write axis 1 specifier to axis 2 variable (variable offset in register 5)
                                        ;   X command output = X PID terms + X feed-forward terms + Y command output
                or 
               AL-1,2WW@5               ; Write negative axis 1 specifier to axis 2 variable (command signal will be subtracted)
                                        ;   X command output = X PID terms + X feed-forward terms - Y command output
                                        

Changes for Rev. 2.6a
===============================================================================
 9/7/04    Added PWM output capability for servo axes. This feature is enabled
           by issuing the Output Mode (OM, code=216) command with a parameter
           of 2 or 3 to a servo axis. This switches the Unipolar Direction
           output signal for that axis to a PWM output. These outputs have open
           collector drivers and may require pull-up resistors to be compatible
           with external circuitry.

           The frequency of the PWM outputs can be changed with the Set PWM
           Time Konstant command (PK, code=204). This command sets the
           PWM frequency for all 4 axes, so no axis number is specified with
           the command. The integer command parameter should be calculated
           as the desired frequency divided by 610 Hz. The default PWM
           frequency is 19.53 KHz.

           Issuing the Output Mode command with a parameter of 2 places a
           servo axis in bipolar PWM output mode. When the motor is at its'
           target position, the PWM output will have a 50% duty cycle. The
           duty cycle will increase or decrease in order to drive the motor in
           either direction. The limits of the duty cycly can be set with
           the Set torQue (SQ) command. This command has a parameter range
           of 0 to 10, which translates to a 0 to 100% duty cycle.

           Issuing the Output Mode command with a parameter of 3 places a
           servo axis in unipolar PWM output mode. When the motor is at its'
           target position, the PWM output will be off. The duty cycle will
           increase from 0 to 100% to drive the motor. The direction of the
           motor is controlled by a separate signal which is configurable.

           When a servo axis is configured to have PWM outputs, the axis
           may be placed in Torque Mode with the QM command. The output
           duty cycle can then be set with the Set torQue command. This
           mode of operation can be used to facillitate testing of the output
           driver circuits.
                                        

Changes for Rev. 2.7a
===============================================================================
 9/9/04    Added New Priority (NP, code=252) command to allow the priority of
           foreground and packground tasks to be adjusted. The parameter to this
           command can be an integer from 11 to 255. Setting a tasks prioroity
           to 11 will give it the highest priority; setting it to 255 will
           give it the lowest priority. This command will only change the
           priority of the task that executes the command. The 2 foreground
           tasks that process commands from the ASCII and Binary interfaces have
           a default priority of 100. All new background tasks created with the
           Generate Task command also have a default priority of 100. With the
           current firmware, setting a tasks priority below either of the
           foreground tasks priorities, will prevent it from getting any run
           time.

 9/23/04   Reduced timeout period for ADC reading in TA and GA commands. New
           counter constant results in a timeout period of approximately 100
           microseconds. Previous code timed out in 1 millisecond. If
           ADC does fail to complete conversion, motor update will still
           have sufficient time to run. Also changed code so that if ADC
           times out, a value of -1 will be placed in the user register instead
           of the bad ADC reading.

 10/4/04   Modified FPGA stepper circuit so that the position counter
           increments at the midpoint of each step cycle. This is where the
           stepper output goes inactive (high). This change insures that the
           stepper output goes to the inactive level after the last step of
           a move. In the previous stepper circuit implementation, the pulse
           counter would increment at the start of the step cycle. If the pulse
           period was sufficiently long, the code would set the At Target flag
           when the motor finished a move, and then stop the stepper pulse
           timer. This would cause the stepper output to remain active (low).

 10/4/04   Added code to enable the breakpoint circuit when a move is initiated
           on a stepper axis. This insures that the breakpoint circuit disables
           pulses when the target is reached. In previous code, the breakpoint
           circuit was enabled in the motor update code after pulses were first
           enabled. If the move was very short, and the pulse rate very high,
           the target could be passed before the breakpoint was enable. See the
           code in stepper_pos_move_start() function.

 10/6/04   Corrected tst_output macro in motifc.h file. This macro is not
           currently used, but it incorrectly read the output register of the
           FPGA that is write only. New version of macro reads the RAM based
           variable that shadows the output register contents.


Changes for Rev. 2.7b
===============================================================================
 10/22/04  Fixed code in timer0_isr routine which test for timer interrupt
           status bits being cleared. The way it works, after writing a 0
           to the timer interrupt status register, the processor waits for
           the interrupt status bits to be cleared. This is done to prevent
           the timer from generating another interrupt immediately. In
           the previous code, all 3 interrupt status bits were being tested,
           not just the one for the timer mode being used. If one of the
           unused status bits became set after the write, the processor became
           stuck in the loop. In the new code, only the interrupt status bit
           for the timer mode being used is tested. There is also a new loop
           counter that will cause the processor to write the register again,
           if the status bits have not cleared after 10 reads.


Changes for Rev. 2.8a
===============================================================================
 11/1/04   Changed code for RT-3 command (Reset) so that motor update task
           is left running while RTEMS monitor is started. This will freeze
           the command interpreters and background tasks but allow motors
           to hold their current position or complete any current motion. The
           RTEMS monitor can be used to determine the current state of all
           tasks. Issuing the GO command to the RTEMS monitor will allow the
           command interpreters and background tasks to resume operation.

           Changed RTEMS monitor task priority to 11 so that motor update
           task will run properly when the RT-3 command is executed.

 11/1/04   Fixed variable name for posdband. Prior code used "dband" as
           name. New code uses "posdband" as described in Help listing.

 11/1/04   Added utgtdelay to list of motor table variables that can be
           accessed with the Look Up (LU) command. This is the variable that
           is set with the Delay at Target (DT) command. This variable is
           named "TGTDELAY" and is a double value in units of seconds.

 11/1/04   Created uoutoffset variable in motor table to store output
           offset value in user units. Internally the controller uses
           outoffset variable that holds the value in controller units.

           Added uoutoffset to list of motor table variables that can be
           accessed with the Look Up (LU) command. This is the variable that
           is set with the Output Offset (OO) command. This variable is
           named "OUTOFFSET" and is a float value in user units (volts).

 11/1/04   Added uoutdband to list of motor table variables that can be
           accessed with the Look Up (LU) command. This is the variable that
           is set with the Output Deadband (OB) command. This variable is
           named "OUTDBAND" and is a float value in user units (volts).

 11/1/04   Added "PK" to the list of parameter commands displayed with the
           Help command. This refers to the new PWM time constant command.

 11/1/04   Changed User Scale, User Zero, User Offset, and User Rate
           commands so that new value will be written to working variables
           in motor table if motor is off when command is issued. If the
           motor is on, the new value will only be written to a temporary
           variable and won't be used until after the motor on command is
           issued.

           Changed motor update code so that command count variables are
           not calculated when axis is off. This caused a problem when user
           scaling is changed and optimal position in old units is multiplied
           by new scaling factor. In worst case, calculated command count
           is larger that 2 billion and floating point exception (watchdog
           trip) occurs. This may have also been a problem in previous code
           after changing the user scaling, and issuing the motor on command.
           In new code, the code for the motor on command now calculates
           the initial command count values using the new scaling factor.
           These values are then used in succeeding motor updates.

 11/1/04   Changed User Scale command so that a parameter of 0 will generate
           an error message and the scaling factor won't be changed. Did the
           same for User Rate command.


Changes for Rev. 3.0a
===============================================================================
 11/1/04   Upgraded to RTEMS release 4.6.2, GCC 3.4.1, Binutils 2.14, and
           Newlib 1.12.0. Code is now maintained as 2 patches to the generic
           RTEMS code. The first is a patch containing a Board Support Package
           (BSP) for the Toshiba RBTX4925 evaluation board and the TX4925
           CPU. The second patch contains a BSP for the MFX-PCI1000. This
           BSP uses the TX4925 CPU components from the first patch. It is
           expected that this upgrade will not change the operation of the
           MFX board.

 11/1/04   Set CPU_ALL_TASKS_ARE_FP true in mips cpu.h file. This causes all
           RTEMS tasks (except the idle task) to be created with the floating
           point attibute set. This was done to prevent FPU exceptions from
           occurring whenever the printf() function is called in a RTEMS task.
           Doing this was safer than trying to ensure that every task using
           printf was created with floating point enabled.
           
           Set CPU_INLINE_ENABLE_DISPATCH true in mips cpu.h file. This was
           done in the previous RTEMS 4.5.0 release to improve task switching
           times; and duplicated in RTEMS 4.6.2 in order to maintain
           performance level.
           
           Changed CONFIGURE_TEST_NEEDS_CLOCK_DRIVER definition in system.h to
           CONFIGURE_APPLICATION_NEEDS_CLOCK_DRIVER. This was done to match
           its use as an application build switch. The same was done for
           CONFIGURE_TEST_NEEDS_CONSOLE_DRIVER, it was changed to
           CONFIGURE_APPLICATION_NEEDS_CONSOLE_DRIVER.           

 11/1/04   Removed code from start.S that placed the processor in uncached
           instruction space before invalidating the instruction cache. This
           appears to be unnecessary, and left the processor running out of
           slow uncached memory for the kernel initialization.

 11/1/04   Moved ASCII Mailbox Character I/O routines from init.c to
           console-io.c. This allows RTEMS to be built for the mfxpci1 BSP
           and not have link errors in the "sample" programs. Added
           code to bsp.h for the mfxpci1 BSP that provides a stub
           set_ascii_ci_busy() function for use with the sample programs.
           For this to work, also had to move the "#define CONFIGURE_INIT"
           statement in the init.c files of the Minimum and Loopback
           samples.

 11/1/04   Move "packed" compiler attribute in data structure declarations
           so that they are compatible with latest GCC compiler. In previous
           code, attribute was placed after the "struct" keyword. In new code,
           attribute is placed after the structure member declarations.

 11/1/04   Changed macros in motifc.h that read and write I/O registers in
           FPGA. Code generated by latest GCC compiler assumes data in
           "packed" structures is unaligned. This would result in code that
           incorrectly accessed the FPGA 16 bit registers one byte at a time.
           New macros cast the address of the FPGA registers as pointers to
           16 bit words, and uses the pointers to directly access the
           registers as 16 bit targets.
           
           Also created macros in motifc.h for accessing the on-board
           Analog to Digital Converter (ADC) through the FPGA registers.
           Changed the code in anacmd.c to use the new macros. This code
           should operate identically to the previous implementation, it's
           just easier to read and maintain.

 11/1/04   Changed get_task_ids() function to be compatible with RTEMS 4.6.2
           code. This function is used by the Information Display command
           to fill an array with background task ID's. In the new version
           of RTEMS, the structure of the _Objects_Information_table has
           changed. The function code was changed accordingly. Also had to
           change the code in the function which compares object names.

 11/1/04   Changed code for Reset command in misccmd.c. New code calls clock
           driver Clock_exit() function to disable clock interrupts. Previous
           code used disable_hbi() function which has been replaced by clock
           driver function.

 11/1/04   Changed RTEMS make configuration file to build code with -O GCC
           optimization. This results in code that provides the highest speed
           performance and closely matches the performance of previous RTEMS
           code.
           
           Added "--srec-len=80" option to objcopy command line to force
           firmware S-record file to have a maximum string length of 80
           characters.
           
 11/1/04   Changed code for Shift Left and Shift Right commands in regcmd.c.
           Previous code will not work with new GCC compiler because "cast
           statements are no longer supported in lvalues". Same for code
           in rwcmd.c that implements Read Byte, Read Word, and Read Long
           commands.

 11/1/04   Modified round() function so that it uses the Round instruction
           in the FPU if available. Otherwise, the rint() function in the math
           library is used. The rint() function rounds a double to the nearest
           integer value, and returns it in a double format. The double is
           then cast to an integer. The new code should run a bit faster.
           
           Moved round() function from tellcmd.c file to motupd.c file.
 
           Added call to round() function in motor update code when converting
           servo output command to integer DAC value. This should produce a
           more precise analog command output. The round() function is already
           used for the stepper output command.

           Replaced calls to rint() and rintf() in command executor with calls
           to round() function. Replaced calls to rint() in tell_prec_double()
           function with calls to round() function. This function is used by
           many of the reporting commands.


Changes for Rev. 3.0a
===============================================================================
 5/5/05    Implemented MCCL file commands: FO, LO, DL, TY, and RF .
 
 5/5/05    Implemented G-code interpreter and supporting commands.

 
Changes for Rev. 3.1a
===============================================================================
 6/20/05   Added GRINDER machine type in G-code interpreter. This machine
           has tool compensation in the YZ plane.
 
 6/24/05   Added support for A, B and C rotary axes.
 
 6/24/05   Eliminated use of B word to cause Auxiliary function macro to be
           called. B word is now used for axis B dimension. Removed
           configuration variable AUXILIARYFUNCMACRO.

 
Changes for Rev. 3.2a
===============================================================================
 7/1/05    Corrected backlash compensation code so that target count is now
           correctly calculated when move commands are executed. Previous code
           used direction of previous move and incorrectly calculated the
           target count.
            
 7/1/05    Enabled Backlash Compensation commands (BD, BN, BF) for stepper axes.

 7/6/05    Modified motor update code for open loop stepper motors. In new code,
           the contribution from the PID to the output command is limited to the
           current set torque value. The feed-forward component of the output
           command is not limited to the set torque value. This allows the Set
           Torque command to limit how fast the stepper motor changes position
           when compensating for backlash. When used for an open loop stepper
           axis, the units of the Set Torque command parameter are as follows:
           
           Speed Range          SQ units
           =========================================
           High                 1000000 Steps/Sec/Unit
           Medium               125000 Steps/Sec/Unit
           Low                  15625 Steps/Sec/Unit
           
           Note: The Set Torque command will only work for an open loop stepper
           axis if the PID parameters have been unlocked. This is done by
           issueing the Input Mode (IM) command to the axis with a parameter
           of 128.


Changes for Rev. 3.3a
===============================================================================
 7/11/05   Added code to cause a wait for motors to stop when a Dwell (G04)
           preparatory code appears in a part program.

 7/11/05   Added code to motor update function to calculate current velocity in
           user units and store it in ucurvel variable. Changed code for Tell
           Velocity and Information Display commands so that they use ucurvel
           variable instead of calculating current velocity from curvel variable
           on the fly. Note that Look Up command for "CURVEL" variable returns
           offset of ucurvel variable which is now updated properly.

 7/19/05   Implemented the following CNC variables:
 
            Variable    read/write   Description
            ====================================================
               1 - 33      r/w       Local variables
             100 - 999     r/w       Common variables
                1000        r        All 32 digital input channels (bit 0 = channel 1, bit 1 = channel 2, ...)
            1001 - 1032     r        Individual digital input channels (1001 = channel 1, 1002 = channel 2, ...)
                1100        r        All 32 digital output channels (bit 0 = channel 33, bit 1 = channel 34, ...)
            1101 - 1132    r/w       Individual digital output channels (1101 = channel 33, 1102 = channel 34, ...)
            2000 - 2999     r        D & H Tool compensation values (2001 = H geom. 1, 2201 = H wear 1, 2401 = G geom. 1, 2601 = G wear 1, 2002 = H geom. 2, ...)
            5001 - 5015     r        Block end position (X=5001, Y=5002, Z=5003, A=5004, B=5005, C=5006, U=5007, V=5008, W=5009)
            5021 - 5035     r        Machine coordinates (X=5021, Y=5022, Z=5023, A=5024, B=5025, C=5026, U=5027, V=5028, W=5029)
            5041 - 5055     r        Work coordinates (X=5041, Y=5042, Z=5043, A=5044, B=5045, C=5046, U=5047, V=5048, W=5049)
            5081 - 5095     r        Tool length compensation value (X=5081, Y=5082, Z=5083, A=5084, B=5085, C=5086, U=5087, V=5088, W=5089)
            5201 - 5215     r        Work offset current values (X=5201, Y=5202, Z=5203, A=5204, B=5205, C=5206, U=5207, V=5208, W=5209)
            5221 - 5235     r        Work offset 1 values (X=5221, Y=5222, Z=5223, A=5224, B=5225, C=5226, U=5227, V=5228, W=5229)
            5241 - 5255     r        Work offset 2 values
            5261 - 5275     r        Work offset 3 values
            5281 - 5295     r        Work offset 4 values
            5301 - 5315     r        Work offset 5 values
            5321 - 5335     r        Work offset 6 values

           Note: variables #1 - 33 and #100 - #999 are located so they
           can also be accessed as MCCL user registers 1001 - 1033 and
           1100 - 1999 respectively. In other words, if a G-code part
           program stores something in variable 100, it is available to an
           MCCL macro in user register 1100. If the MCCL macro stores something
           in register 1101, the part program can access it in variable 101.


Changes for Rev. 3.4a
===============================================================================
 7/21/05   Fixed tool compensation so that finish position of a line followed
           by an arc is correctly calculated for lathes and grinders. In
           previous code, the compensation algorithms were using the start
           position of the line that included the tool offset values. To
           work properly, the algoritms needed to use the start position
           without the tool offsets. In order to accomplish this, created
           a new set of variables that hold the "compensated and offseted"
           positions: coxstart, coystart, cozstart, coxfinish, coyfinish,
           cozfinish. The compensation algorithms use just the compensated
           positions without the offsets.


Changes for Rev. 3.5a
===============================================================================
 7/25/05   Changed wait_stop function in G-code interpreter so that it only
           waits for axes that are in position or contour mode. This allows
           auxiliary axes to be run in velocity mode and not stall G-code
           execution.

 7/25/05   Added code to reset motor positions in the block queue after a
           M-code causes a MCCL macro to be called. In previous code, if the
           MCCL macro moved a motor, the G-code interpreter might not initiate
           a succeeding motor move.

 7/25/05   Added run_abort and run_active flags to run status variable.
           These flags will be accessible with the Tell Run Status and
           Get Run Status commands. The run_abort and run_active flags
           will be bits 24 and 23 respectively.
 
 7/25/05   Changed GRS command to place run status value in accumulator (user
           register 0). Previous code placed address of runstatus variable
           in accumulator.

 7/25/05   Modified code for Run Terminate (RUT) command to accept a parameter
           of -1. In previous code, issuing the command with no parameter
           caused the run_abort flag to be set, and the command to wait
           until the G-code interpreter terminated (run_active flag cleared).
           In the new code, issuing the command with a parameter of -1 will
           set the run_abort flag and the command will return immediately
           without waiting for the G-code interpreter to terminate.


Changes for Rev. 3.6a
===============================================================================
 7/27/05   Fixed code so that B axis will perform linear interpolated (G01)
           moves. Previous code set vword flag instead of bword.

 7/27/05   Crested post blocks to support improved tool compensation
           implementation. Current code does not use them. Reduced number
           of possible pre-blocks from 3 to 2. Tool compensation will not use
           more than 2.

 7/27/05   Added code to print end positions of pre-blocks and post-blocks
           that are executed.


Changes for Rev. 3.7a
===============================================================================
 7/28/05   Modified Escape Task command so that a parameter of 0 will cancel
           all background tasks.

 7/28/05   Added new system variables for G-code interpreter:
            Variable    read/write   Description
            ====================================================
                6001        w        Tool compensation type (0 = Type A, 1 = Type B (default)) 
                6002        w        Display pre-block text (1 enables, 0 disables (default))
                6003        w        Display post-block text (1 enables, 0 disables (default))
            6101 - 6115     w        Disable wait stop checking (1 disables, 0 enables (default))
                                        (X=6101, Y=6102, Z=6103, A=6104, B=6105, C=6106, U=6107, V=6108, W=6109)
           Added code to initialize these system variables at the start of
           a part program.

 8/2/05    Improved implementation of tool radius compensation in G-code
           Interpreter. New code will generate path that avoids clipping
           corner of block following compensation startup block. This is
           also done for corner of block that precedes compensation cancel
           block. This implements Type B tool radius compensation for
           startup and cancel blocks. Previous code only supported Type A.


Changes for Rev. 3.8a
===============================================================================
 8/15/05   Fixed arc moves in G-code interpreter. Code changes in revision 3.4a
           caused arc center position to not be set correctly.

 8/15/05   Added 2 system variables to G-code interpreter to control filling
           of motion buffer:
            Variable    read/write   Description
            ====================================================
                6004        w        Enable increment test (1 = enables, 0 disables (default)) 
                6005        w        Motion buffer fill count (integer between 2 and 250)
           When enabled, the G-code Intepreter will check the change of direction
           between successive motions. If it is less than the specified
           Increment value, the motions will be combined in the motion table.
           The Motion Buffer Fill Count sets the maximum number of motions
           that will be placed in the buffer.


Changes for Rev. 3.9a
===============================================================================
 8/18/05   Modified G-code Interpreter operation so that display of block text
           is in sync with block execution. Also created global variables
           to hold the status of the block currently executing. These variables
           are used by the status reporting commands. In the previous code,
           the status values came from the block structure that was modified
           as soon as the block executed (before finishing motion).


Changes for Rev. 4.0a
===============================================================================
 8/24/05   Added new variable PIDTRQ to the motor tables. This value is used
           to limit the contribution of the PID term to the output torque.
           Created Torque Limit command (QL, code=199) to set the value of
           the variable.
           
           Remove code from pid_calc() function that applied torque limits
           differently for open loop steppers. New code treats all motor
           types the same.
           
           Note: The Torque Limit command will only work for an open loop stepper
           axis if the PID parameters have been unlocked. This is done by
           issueing the Input Mode (IM) command to the axis with a parameter
           of 128.


Changes for Rev. 4.1a
===============================================================================
 9/26/05   Migrated code to latest release of RTEMS, 4.6.4

 9/28/05   Changed build to implement the Timer_initialize() and Read_timer()
           functions. These functions are used by the RTEMS Timing Test Suite.
           All BSP's that use the Toshiba TX49 family of MIPS processors will
           now use the timer code that is included in the MIPS libcpu
           directory. This code uses the timer that is part of the System
           Control Coprocessor. The clock rate of this timer is 1/2 of the
           CPU clock rate.
     
 9/29/05   Corrected code in mips_vector_isr_handlers() function that
           determines proper interrupt vector number. In previous code,
           depending on what interrupt mask bits were set in the Status
           register, the wrong interrupt service routine could be called.

 9/30/05   Modified contouring operation so that the target position is
           updated with the optimal position whan the controlling axis is
           commanded to stop. In previous code, target and optimal positions
           were updated with the current true position. This allowed the
           target and optimal positions of the axes to shift after they
           stopped.

 9/30/05   Added "confidential and propietary" notice to all PMC source files.


Changes for Rev. 4.1b
===============================================================================
 10/7/05   Fixed calculation of feed-forward term for slave axes. This required
           adding a new variable called Current Speed (curspd) to motor table.
           In previous code, sign of feed-forward term was not correct for
           slave axes in contour mode. Current velocity is now a signed value
           that indicates current direction of travel.

 10/7/05   Added code to zero Curacc motor table variable in Motor On command.
           This was done for consistancy in code.


Changes for Rev. 4.2a
===============================================================================
 10/12/05  Implemented fast timer to record the amount of time spent performing
           the motor update. Latest value, maximum value, and minimum value
           can be read by issuing the Information Display (ID) command with a
           paramter of 8. Values are displayed in microsecond units. Each
           time the ID8 command is executed, the maximum and minimum values
           are reset.

 10/14/05  Migrated code to latest release of RTEMS, 4.6.5


Changes for Rev. 4.3a
===============================================================================
 11/11/05  Added support for MFX-PCI1802 version of the controller. This is an
           8 axis servo controller. All 8 axes use PWM outputs for the command
           signal. While this product is specified to not have the 4 channels
           of analog output, if the DAC is present the software can use the
           analog output to command the first 4 axes.


Changes for Rev. 4.4a
===============================================================================
 7/20/06   Added code to initialize variables used in PID calculations during
           execution of Motor On command. This elliminates glitch in servo
           command output when motor is turned on after a following error.


Changes for Rev. 4.5a
===============================================================================
 7/31/06   Added support for MFX-PCI1262 version of the controller. This is a
           2 axis servo, 6 axis stepper controller. Axes 1 and 3 are configured
           as servos, 2, 4, and 5 through 8 are configured as steppers.

 7/31/06   Corrected macro used to read capture register in FPGA. The
           read_capposition() macro in previous code read the Idxcapbp element 
           from the motor interface structure. New code reads the Poscmp
           element. In all previous FPGA configurations, reading Idxcapbp
           produced same results as reading Poscmp. In the FPGA configuration
           for the MFX-PCI1262, this is not the case and the macro needed to
           be corrected. Renamed structure elements from idxcapbp and poscmp,
           to idxbp and capcmp repectively. This reflects register functions
           accurately.

 7/31/06   Added code to record and display the motor update period. This is
           the time between motor updates. This value can be displayed along
           with the time to perform the update, with the Information Display
           command (ID8).


Changes added from Custom Version LA1 to PM1 Rev. 4.5a
===============================================================================
 8/1/06    Increased timer interrupt rate to 8 Khz. Servo High Speed rate will
           be 8 Khz, Medium 4 KHz, Low 2 KHz. Trajectory generators and stepper
           axes will be at 1 KHz rate.
           
           
Changes for Rev. 4.6a
===============================================================================
05/27/07   Added new parameter to Input Mode (IM) command to allow changing default
	   polarity of home sensor input edge detection during execution of 
	   Latch Edge (LE) controller command.  Default was rising edge for 
	   normally-open switches.  Asserting bit 4 (i.e. IM(8)) in the mode 
	   register has the effect of changing the polarity to falling edge for
	   normally-closed switches.

11/15/07   Added support for MFX-PCI1442 version of the controller. This is a
           4 axis PWM servo, 4 axis stepper controller. Axes 1 thru 4 are configured
           as servos, 5 thru 8 are configured as steppers.  The distinction to 
           this board is the distribution of axes on each connector:
           
           	J1:	Axis 7
           	J2:	Axis 8
           	J3:	Axes 1 2 5
           	J4:	Axes 3 4 6
           	
	   This architecture was developed to allow a 1440-type controller
	   board to be created from lower-cost 1040-2 hardware by using the
	   stepper encoder inputs for the servo axes.  In addition, the
	   customer can have 6 axes on only two connectors in this configuration.
	   
Changes for Rev. 4.6b
===============================================================================	   
	   
01/08/08   Added support for hardware high-speed strobe function for MFX-PCI1440
	   (stepper axes only) and MFX-PCI1040 versions of the controller. 
	   This feature extends the capability of the compare circuit by providing
	   a new OC mode 5 that produces a set of strobe pulses starting at the
	   axis compare position.  Rather than a firmware-mediated set of pulses,
	   the fpga now produces a train of strobe pulses at regular encoder count
	   intervals.  

           The MCConfigureCompare() and MCEnableCompare() functions, as well
           as the corresponding MCCL calls were expanded to support the
           additional fpga registers required for this function.  The following
           sequence of commands illustrates the revision:
           
           1OC5       // set output compare mode to 5 for hardware strobe function
	   1LC1000    // set compare start position to 1000 counts
	   1NC400     // set PW = 10 uS (25E-9 * 400)
	   1OP10      // set strobe period to 10 encoder counts
	   1BC100     // start compare and issue 100 strobe pulses
	   
04/01/08   Modifications to strobe circuit

		- function will only exist on 1040 and 1440 stepper axes
		- logic modified to drive strobe circuit from encoder inputs
		  only, for both open and closed loop  modes
		  		
Changes for Rev. 4.6c
===============================================================================	   

02/23/08   More modifications to strobe circuit driven by customers who want 
	   high-speed strobe output on servo axes
	   
	   	- 1040 has strobe logic on axes 1-4
	   	- 1440 has strobe logic on axes 1-2-5-6
		
Changes for Rev. 4.7a
===============================================================================	   

03/12/09   Implemented new 1622 board architecture.  This board type has the
	   following axis configuration
	   
	   axis			type	
	   
           1-4			PWM servo		
	   5-6			Step/Direction pulse		
           7-8			PWM servo		

	   A single configuration file was created that is based on the 1802
	   board type containing 8 encoder channels, by definition.  The only
	   available configuration will be 1622_2_e with ADC.

03/30/09   Implemented a 1400 board configuration which has 4 servos only.  The
	   two configuration types (-0 and -2) have axes 5-8 disabled.  The o/s
	   loads a 1440 fpga image for this configuration.
	   
Changes for Rev. 4.8a
===============================================================================	   

05/18/10   Added support for 8 kHz interrupt (PID) rate, providing partial 
	   compatability with 16 kHz version of MFX-ETH.  The 200 MIPS 4925
	   processor cannot support the higher interrupt rate.  The following
	   commands are now supported by the MFX-PCI:
           
           	YL	low interrput rate (4 kHz) default
           	YM	medium interrupt rate (8 kHz)
          
07/26/10   Problem was reported on pulse axes in s-curve profile mode where axis
           was stalling one count short of target without assertion of At Target
           and Trajectory Complete.  The PID code was modified to remove the one
           count pulse axis deadband for open-loop steppers in s-curve mode only
           to resolve the problem.
           
07/28/10   Modified logic in micwcc.v to address problem in gantry mode on pulse axes.
           The slave axis pulse count was found to be incorrect in almost all position moves.
           This was traced to the lack of implementation of the breakpoint latch, relying
           instead on position error and velocity to terminate the move.  The fix involved
           adding muxes to all stepper interfaces that allowed the slave axis step and
           direction outputs to be identical to those of the master axis.  The SM command
           was modified to write a 2-bit mux select to a new fpga register in the slave axis
           which switches in the signals from the master axis.
           
Changes for Rev. 4.8b
===============================================================================	   

10/15/10   Added new command to specify fixed min/max velocity ratio for pulse axes. 

			aVRn		Velocity Ratio = n (double)
			(function 309)
			
			mtr->velratio	motor table variable (added to lookup)
			
	   The ratio defaults to 0 in which case the MV and SV commands work as always.  If
	   mtr->velratio is set to a non-zero value, MV returns without changing the minimum
	   velocity.  The minimum will instead be set based on the min/max ratio and will 
	   track changes to the SV and VR commands.  When the ratio is set back to zero,
	   the previously programmed value for minimum will be restored.
	   
10/18/10   Added parameter checking to SM and SS commands that will only allow hardware 
           muxing of pulse output on slave axis (07/28/10) if the slave ratio is 1.  This
           provides accurate gantry operation but still allows gearing for other applications.
           
10/23/10   Fixed bug that was preventing pulses from being re-enabled when an axis changed from
           a slave ratio of 1 to any other value.  This was a result of the recent changes to
           the SS command to support the pulse axis gantry multiplexing,    
	   		           
	   		           
Changes for Rev. 4.8c
===============================================================================	   

07/22/11   Bug fix for spline contouring when using synchronized motion.  It was
           found that a zero-length move resulted in divide-by-zero fpu exception
           and a crash.  This was fixed in pre_process_spline() in ctrcmd.c

Changes for Rev. 4.8d
===============================================================================	   

09/22/11   Bug fix for servo axis high-speed strobe compare function.  The direction
           of motion was not being considered in the encoder count logic resulting
           in incorrect strobe output position.  This was fixed in strobe.vhd (motifc_lib).
           
09/27/11   Deleted support for all higher-speed loop rates.  Apparently the interrupt
           timer overhead was an issue for some high performance systems and 
           produced noticable perturbation.  Everything reverts back to 4 kHz PID rate.
           
10/04/11   Beta release of enhancement to high-speed strobe logic that supports 
           bi-directional position moves (previously only + motion).  Also modified
           the state machine to eliminate a spurious 25 nS pulse at the end of the
           programmed strobe output.
           
10/13/11   Management of the beta release caused the incorporation of the older
           revision of clock interrupt driver and associated 16 kHz PID loop rate
           support (deleted on 09/27).  The source trees were resolved and correct
           versions of libbsp functions and init() functions now insure that the
           controller supports only 4 kHz PID rates, as intended
           
Changes for Rev. 4.8e
===============================================================================	   
11/30/11   Implemented a 4-channel PWM controller for the 1040 platform.  The
           outputs are placed on general-purpose digital outputs as follows:
           
           	PWM channel		   Digital Out (channel)
           	     1				10 (42)
           	     2				11 (43)
           	     3				14 (46)
           	     4				15 (47)
           	     
           The digital outputs are still available for use if the PWM circuit is 
           disabled.  The duty cycle of each channel is independent but there is a
           common clock and prescaler used by all 4 channels.  
           
           The two command mnemonics that are used to control these circuits are:
           
           	PKn		   -	set PWM frequency 
           				(f = n * 50 Hz)
           	
               aPGn                - 	set duty cycle of channel a
	       (function 183)	  	(duty cycle = n / 65535)
				
	   Notes:
	      	1. To disable the PWM circuit, command a duty cycle of zero
	   	to the desired channel (aPG0).
	   
	   	2. The base frequency of 50 Hz is approximate (50.86 Hz)
	   	
12/05/11   The Spartan2 DLL allows fewer frequency synthesis options so in order
           to maintain compatability between PCI and ETH versions, the base
           frequency of the PWM circuits had to be changed.  The new value is 
         
         
           	PKn		-  set PWM frequency 
           			   (f = n * 38 Hz)      
           			
	   It was also noted that a frequency scaler value that is an exact
	   power of 2 (8, 32, 1024,...) results in a more jitter-free pulse
	   train.  At other values and high frequencies, the jitter can be as 
	   great as 500 nS.  This will be addressed and fixed in a future release.
	   
12/08/11   Implemented Position Following Error Limit feature to allow user to 
           specify an allowable interval during which the axis exceeds the programmed
           following error.  This is useful for excursions outside the limit during
           accel and decel that may not be as of much interest as constant-velocity
           error.  The new function is
           
           	aFXn  			-   sets axis a to a following error time
           	(function 169)    	    limit to n mSec before asserting the error
           				
           The motor variables that can be looked up are:    
           
           	poserrcnt (int)		PID loop error counter
           	poserrlim (int)		position error limit (loop counts)
           	poserrtime (long)	position error limit (mSec)	   
           	
	   Changed function number of VR command to eliminate conflict with 
           piezo mode functions that will likely be merged into the PM1 code           	
	   	           
01/24/12   Implemented OEM customizable version string reported by VE command.  
           This required the following addition to the fwconfig structure
           and generation of new configuration files for the boot rom
           
           typedef struct 
           {
	   	unsigned short modelnumber;
	   	unsigned short sspare1;
	   	unsigned short maxaxisnum;		
	   	unsigned short sspare2;
	   	char oemmodel[64];			/* OEM model number string */
	   	char oemname[64];			/* OEM company name string */
	   	int ispare[30];
	   	MFX_AXIS_CONFIG  axisconfig[8];		
	   } PACKED MFX_FIRMWARE_CONFIG;

	   The new string fields are populated with the default PMC information during
	   boot rom creation, but at controller startup, the strings can be re-written
	   with OEM-specific data.  Also, the VE command was modified to report these
	   strings instead of the previous hard-coded data.

01/27/12   Implemented a 32-bit counter register that can be used by applications
           as a semi-realtime clock.  This was implemented on the 1040 platform only
           but may migrate to others if there is a demand.  The offset of the register
           that returns the integer clock count is:
           	
           		0xb8000140	

Changes for Rev. 4.8f
===============================================================================	   
04/12/12   Implemented Data Logging function on MFX-PCI to allow improved visibility
	   into real time events, failures, etc.  The first iteration of this feature
	   will have fixed debug events coded into the embedded system but subsequent
	   versions will have a more dynamic mechanism for identifying log data. An 
	   additional MCCL function was required to control the data logging.
	   	   
		aEGn (function 254) - enable/disable data logging per axis
		
					a = axis (0 => all axes)
					n = 0 disable logging
	 				   -1 reset log buffer to initial values
	 				    1 enable logging
	 				    
	   
	   Comprehensive status information can be logged by setting flags contained 
	   in the higher-order bits of the n parameter to the EG command above.  The flag
	   bits and their significance are as follows:
	   
	   	n |= 0x8000 - 	log all Move commands in position mode
	   	 		log all position move completion events 
	   	
	   	n |= 0x4000 - 	log all Move commands in contour mode
	   			log all contour move completion events 	
	   			
	   	n |= 0x2000 - 	log all Move commands in slave mode
	   			log all slave move completion events 		   			
	   	
	   	n |= 0x1000 - 	log each point from profiler
  	
	 			    
	   The function call to insert an event in the status log is
	   	   
	   	void log_stat(char *stat_str, int cnt, int axis)
	   	
	   		stat_str 	status log message (\n termination)
	   		cnt		message length
	   		axis		axis number
	   		
	   		
	   The message will be logged with a time stamp followed by the axis identifier and
	   the message string.  Following is a description of the data structure related to
	   event logging.		    

			#define STATLOGSIZE 0x1000
			#define STATLOGNUM 2
	
			typedef struct {
			int stat_log_num;			/* number of buffers */
			int stat_log_size;			/* size of buffers */
			char *stat_log_addr;			/* base address of buffer space */
			char *stat_log_start[STATLOGNUM];	/* pointers to start of buffer data */
			char *stat_log_end[STATLOGNUM];		/* pointers to end of buffer data */
			int stat_log_cnt[STATLOGNUM];		/* byte count written to current buffer */
			int stat_log_flg[STATLOGNUM];		/* buffer status flag (full,...) */
			int stat_log_en;			/* individual axis log enables */
			int stat_log_rst;			/* reset from external app */
			char stat_log[STATLOGNUM][STATLOGSIZE];	/* array of log buffers */
			} PACKED STATUSLOG;


	   The data log is statically linked to allow a fixed address in PCI user 
	   space to allow applications to pull data from the controller without the API
	   opening a controller handle.  The offset of the structure is 0xA0021000 (uncached).
	   The offset can be verified by issuing a lookup command for the variable "statuslog".

           	statuslog (char *)		offset to STATUSLOG structure
           
           
Changes for Rev. 4.8g
===============================================================================	   
07/18/12   Corrected defect in OEM version string mechanism from 4.8e.  Without
           a newer configuration file containing the string data, the VE command
           produced blank lines.  A field was added to the config data as follows:

           typedef struct 
           {
	   	unsigned short modelnumber;
	   	unsigned short sspare1;
	   	unsigned short maxaxisnum;		
	   	unsigned short oemid;			/* non-null for new config data */
	   	char oemmodel[64];			/* OEM model number string */
	   	char oemname[64];			/* OEM company name string */
	   	int ispare[30];
	   	MFX_AXIS_CONFIG  axisconfig[8];		
	   } PACKED MFX_FIRMWARE_CONFIG;

	   The oemid field is now checked and if null, a default string is generated
	   by within the VE command. If not, the oem data is taken from the config
	   data and displayed.
	   
Changes for Rev. 5.0a
===============================================================================	   	   
09/15/12   Implemented s-curve trajectory planner based upon trapezoidal accel/decel in addition
           to the current sinusoidal profile.  This mode is selected by calling the exisitng S-curve 
           select function with a non-zero parameter
           
           
           	aPSn		select S-curve profile for axis a
           			n = 0		sinusoidal accel/decel function
           			0 < n < 0.5	trapezoidal accel/decel function ramp = n
           			
           The ramp value is defined as the percentage of the accel time ramping to
           full acceleration.  A value of 0.1 will provide a .1/.8/.1 trapezoid.
           
           The value of this parameter can be determined by the lookup variable
           
           	mtr->scrvramp	(double ramp value)	   
	   
09/18/12   Added DAC scaling/offset capability.  This allows the user to change the dynamic
	   range of the analog servo DAC with console commands.  The default +10/-10 volt 
	   range can be changed by accessing two motor variables:
	   
	   	dacrange (double)	specifies DAC range in +/- volts
	   	dacoffset (double)	specifies DAC offset in volts

	   There is no parameter error checking as the DAC is always clipped at +10/-10

01/08/13   Added ability to invert the Amp Fault input in a manner similar to that used
           to invert limits.  The Amp Fault On function was modified to include a 
           paramater as follows:
           
           	aFNn		axis a Amp Fault on
           			n = 0		normal polarity
           			n = 128		inverted polarity
           			
           The status variable MTRAFI which shows the state of the inversion was
           assigned to AUXSTAT(15).
           	   
02/18/13   Corrected defect in PG command that caused controller to hang due to
           incorrect interrupt enable/disable
           
02/21/12   Implemented the 32-bit counter register and 4-channel PWM controller from
           rev 4.8e on the 1262 platform.  These features are added to various 
           controller types on an as-needed (customer request) basis.  The configuration
           data (mfxconfig) was modified to add the 1262-3 board configuration.        
           
04/24/13   Added new trapezoidal trajectory generator without on-the-fly position
	   change capability.  This was to allow latitude in debug, anomolous
	   stepper behavior, etc.    Only stepper axes can utilize this function by
	   selecting the type of trapezoidal trajectory.  Servo axes will always use
	   the on-the-fly trajectory generator.  The choice of which trajectory generator
	   is dynamically selected, based on the state of the following new motor 
	   variables:
           
           	mtr->otf	otf state flag (selects trajectory generator)
           	mtr->otfmode	otf mode (enable/disable/count-based)
           	mtr->otfcnt     otf count threshold
           	
           An MCCL command, added to support the new variables, and its command
           arguments are as follows:
           
           	aFYn		Trapezoid On the Fly control	(a - pulse axis)
           	(function 307)	
           	

		
		n	mtr->otfmode	mtr->otfcnt	on-the-fly trajectory
		--------------------------------------------------------------
		0	    1		    0            always on
		<0	   -1		    0            always off
		>0          0               n		 on  (move > n)
							 off (move < n)	
							 
	   Usage examples:
	   
	   	5fy0	;axis 5 otf trapezoidal trajectory always selected
	   	3fy-1	;axis 3 non-otf trapezoidal trajectory always selected
	   	5fy100	;axis 5 move distance >100  otf trapezoidal trajectory selected
	   		;	move distance <100  non-otf trapezoidal trajectory selected                      

04/25/13   Revised control methodology of trapezoidal on-the-fly to improve clarity and
           flexibility for future h/w and f/w enchancements.  The motor variables, MCCL 
           command syntax and their effect are as follows:
           
           
           	aFYn		Trapezoid On the Fly control	(a - axis)
           	(function 307)	
           	

		
		n	mtr->otfmode	trajectory generator	on-the-fly mode
		--------------------------------------------------------------
		0	   0		     type 0 		    on
		1	   1		     type 1                 on
		2          2                 type 1                 off
							 
	   
		   
	   The trajectory generators are defined as
	   
	   	type 0:	trprof.c [trapezoidal_trajectory()]
	   		
	   		original implementation of trapezoidal trajectory planner
	   		that was created to support on-the-fly position changes
	   		  
	   	type 1: trprof.c [trap_traj()]
	   		
	   		new parameterized implementation of trapezoidal trajectory
	   	        planner that is more robust and immune to math errors on
	   	        short, high-velocity moves.  This trajectory planner now
	   	        supports on-the-fly moves with the temporary limitation that
	   	        axis stops occur on all commanded position changes.  This 
	   	        slight limitation will be corrected in a future release.
	   	        
Changes for Rev. 5.0b
===============================================================================	   	   
   
04/30/13   Added special board configurations as follows:	

	   1083-2	8 pulse axes	
	   1173-2	7 pulse axes 1 PWM servo (axis 6)
	   1263-2	6 pulse axes 2 PWM servo (axes 1 & 2)
	   
	   All axes have encoder support and pulse axes have hardware master/slave 
	   capability.  Refer to individual pinout documents for I/O details.
	   
05/06/13   Added new motor variables to insure additional  pass through path 
           generator to eliminate spurious enables on STEPENA signal in fpga.
           The variables are
           
           	mtr->stpdly	- specifies number of passes through path
           		          generator after AT latch fires (default = 1).
           		          This value can be inspected/set by a lookup
           		          of "stpdly"
           	
           	mtr->stptimer	- timer variable
           	
           This mechanism is applicable only in mode 1 and 2 trapezoidal trajectory
           planners on open-loop pulse axes.
	   
05/09/13   Corrected a number of bugs related to new trapezoidal trajectory generator
           implementation including
           
           	- incorrect processing of ST command causing resumption of motion
           	- incorrect switching of trajectory modes (trapezoid, s-curve..)
           	
           All fixes involved insuring proper handling of mtr->otfmode variable
           under circumstances not earlier considered.

05/23/13   Added new motor variable "auxposcount" to allow query of auxilliary position counter through 
	   motor table offset lookup.           
	   		
05/23/13   Added new motor variable "auxoffset" to allow query of auxilliary position offset value that
           is modified by the AHn command.
           
05/23/13   Added new motor variable "auxindex" to allow query of auxilliary index position value that
           is modified by the AF command.	   
           
06/03/13   Corrected problem related to stop command issued during position move on
           pulse axes.  The optimal position was not set to the final target position
           after the stop and Trajectory Complete was frequently not set.  This was
           corrected by updating the breakpoint latch target position following decleration
           calculation performed in the ST command function.
   
   
Changes for Rev. 5.0g
===============================================================================	   	   
   
06/13/13   Implemented several corrective measures in firmware to allow the type-2
           Trapezoidal trajectory generator to behave properly under corner conditions 
           such as extremely high or low accelerations and velocities.  In addition, 
           the Stop command was not functioning properly when used in a move-wait-stop
           scenario.  These and other performance improvements and enhancements were made

06/14/13   Modified slave axis behavior to correctly indicate target position of master axis
	   when pulse axes are configured in gantry mode.


Changes for Rev. 5.0h
===============================================================================	   	   
06/18/13  Corrected problem that prevented execution of Stop command in velocity mode
           whe trapezoidal trajectory planner mode 2 was selected.  When velocity mode
           is selected now, type 0 trajectory will be switched in to provide stop
           function.  When position mode is re-selected, the previously selected
           trapezoidal trajectory planner mode will be reinstated.

Changes for Rev. 5.0j
===============================================================================	   	   
06/19/13  Corrected problem that was resulting in incorrect target position following
           execution of stop command in position mode.  Also eliminated the stpdly 
           timer that was used to synchronize TC and AT in the linear path generator.
        

07/16/13  Corrected problem involving stop mode during +/- hardware limit detect
          when in trapezoidal mode 2.  The problem was identical in nature to 
          the one found to effect the ST command where a trapezoidal rampdown
          was not being calculated.
          
Changes for Rev. 5.0k
===============================================================================	   	   
07/27/13  Revised end-of-move behavior under commanded stop conditions to cause axis  
          to set velocity to minvel, rather than 0
          
07/31/13  Implemented delay timer for stepper stop commands that allows for delayed
          pulse to increment position counter thereby updating optimal and 
          target positions correctly.  This is the same variable used in 5.0b for
          all postition move completions that was subsequently deleted. 

08/09/13  Replaced variable delay timer used in stop flag processing with consant
          1-cycle delay.  Did a clean build of RTEMS.
          
Changes for Rev. 5.0m
===============================================================================	   	   
08/15/13   An MCCL command was added to allow programmatic control of unused
           bits in the motor status word
           
           	aSUn		set mtr->status(31:30) to n on axis a
           	(function 138)	

08/20/13   Corrected problem in velocity ratio command.  The profile velocity was not
	   getting updated correctly after the VR command unless a subsequent SV command
	   was issued.
 
 Changes for Rev. 5.0n
===============================================================================	   	   
09/12/13   Added check of stepper direction bit in linear path generator that is 
           intended to address problem of motion away from target due to incorrect
           position determination when on-the-fly moves are issued.

09/17/13   Corrected bug in direction bit check that was disrupting velocity mode.

09/23/13   Revised trajectory calculations in movetopos() that was incorrectly 
           determining times and distances for type 2 trajectories with unequal
           accel and decel values.

 Changes for Rev. 5.0p
===============================================================================	   	   
09/25/13   Revised logic in movetopos() that was being used to determine completion
           of previous move.  Changed qualifier from profiler trajectory complete
           to motor trajectory complete and added additional check for pulse disable.
           
 Changes for Rev. 5.1a
===============================================================================	   	   
10/15/13   Release version 5.1 to indicate viable FY1 on-the-fly functionality.
           This is still a preliminary release which performs on-the-fly moves
           during constant velocity but will hopefully represent significant
           uplift in speed.  A version to manage otf moves during acceleration
           will follow.
                	
 Changes for Rev. 5.1b
===============================================================================	   	   
10/15/13   Implemented feature from bl_4.7 source tree that inhibits execution
           of successive MA commands to the same position (other than 0).  This 
           had been shown to provide significant speed improvement in some 
           applications.

 Changes for Rev. 5.1c
===============================================================================	   	   
10/20/13   Implemented on-the-fly processing for accleration phase of trapezoid

 Changes for Rev. 5.1d
===============================================================================	   	   
10/22/13   Implemented on-the-fly processing for triangular velocity profiles

10/24/13   Corrected error in triangle otf processing whereby max velocity was
           ignored during calculation of new accel/decel times.
           
           Added logic in SA, DS, SV, and MV commands to ignore changes to any
           of these parameters while an axis is in motion if in FY1 mode.
           
           Corrected flaws in EG enable data logging command to conform to original
           behavior desribed in 4.8f

 Changes for Rev. 5.1e
===============================================================================	   	   
11/05/13   Corrected flaw that allowed changes to accel, decel, velocity while
           axis is moving in FY2 mode.  Now, the SA, DS, SV and MV commands
           will be deferred until the axis stops in this mode.

 Changes for Rev. 5.1f
===============================================================================	   
11/11/13   Corrected flaw in linpath() that was causing unwanted direction reversal
           under certain conditions of fractional position moves.

 Changes for Rev. 5.2a
===============================================================================	   
12/01/13   Revised algorithm for processing on-the-fly position changes to correct
           fundamental flaw in triangular profile processing/generation.  
           
           Also revised mechanism to capture otf vel/accel/decel commands but
           have not completed the full implementation in this release.  These
           commands will be defered until the axis stops and then applied.
           
12/12/13   Added MCCL function to control the selection of recording data, and
           changed the recording buffer sizes to 2048.  The new command is
           
           	aDVn		set recording display mux to n on axis a
           			(n = 0    display torque on DQ command)
           	                (n > 0    display velocity on DQ command)
		(function 255)           	   
		
	   The new function is supported by the addition of a velocity recording
	   buffer to the exisiting recording buffers (position, status,...)
	   
 Changes for Rev. 5.2b
===============================================================================	   
01/13/14   Development build that includes logic to record and display statistics
           related to on-the-fly moves.  This includes percentage of otf moves
           that can be processed by controller and the estimated move time
           savings of FY1 mode compared to FY2.  The statistics are displayed
           by entering
           
             	aID9	a - axis number
	   
02/06/14   Revised axis service logic in 4kHz motor update loop.  The rate at
           which pulse axes are serviced was increased from 1 to 2 kHz.  Hardware
           test points show very little latency increase in service routine
           and this seems to improve synchronization of status flags between
           1 and 4 kHz services like trajectory planner, path generator, PID, etc.

 Changes for Rev. 5.3a
===============================================================================	   
04/09/14   Backed out change to motor update service rate on pulse axes and 
           returned to 1 kHz.  Early testing showed some anomolies that were
           related to the rate change and no apparent benefit.
           
04/10/14   Development/test build based on rev. 5.2b with pulse axis service 
           rate set back to the original 1 kHz.  Created separate source branch
           containing on-the-fly statistics which will be used for internal
           testing only.
           
           pm1_5.3a - 1 kHz pulse axis update rate w/o otf statistics
           dv1_5.3a - 1 kHz pulse axis update rate w/ otf statistics           

05/20/14   Revised logic in movetopos() involving suspension of task waiting 
           for axis to stop during on-the-fly direction change.  Deleted condition
           requiring MTRAT to be true in order to determine if this is source
           of MA command not returning (and hanging binary ifc).

05/21/14   Removed all data logging and other test point logic due to some 
           discrepancies seen running the API benchmark test.  This was
           done to try to optimize servicing of the binary command ifc task.

05/23/14   Added MTRAT condition back into wait-for-stop task suspension.  Early
           testing indicates that the older failure to assert PRFTC seems
           to result without it.

06/10/14   Revised movetopos() in direction reversal processing that was causing
           the binary ifc to remain busy during stopping.
           
06/10/14   Added provision to movetopos() that checks for existing stop flag
           active and if so, suspends task until trajectory complete.  This
           if() is followed by if else() clauses to process FY1 moves.  This
           appears to resolve the discontinuity in optimal and target resulting
           from a move->wait->stop->wait->move sequence.

06/16/14   Corrected flaw from 5.4a related to FY1 mode direction reversal.  The
           deceleration parameter calculation had been inadvertantly deleted.

 Changes for Rev. 5.4.0
===============================================================================	   
09/12/14   Added new CNC command "GCV" to get g-code variable.

           Enhanced CNC single work coordinate feature with logic from MFX-ETH
           (includes much larger work offset table size 7 ==> 55).
           
           Version numbering has been changed from a numeric/alpha hybrid (e.g. 
           5.4a) to a pure numeric format with an aditional build number 
           generated out of the version control system (e.g. 5.4.0.32). 
           
           C-Preprocessor is now using C99 standards (more modern features and 
           better code checking).
           
           
==============================================================================
End of Revision History
===============================================================================
            